 
 
READDOS.TXT - BookManager (TM) READ/DOS Version 1.2 Product Information File
----------------------------------------------------------------------------
 
You must read the SOFTCOPY.AGR file before using any IBM softcopy
information.
 
Please consult BookManager READ/DOS: Installation, Getting Started, and
Customization (SX76-0148-0).
 
290K of free memory is the minimum memory required to utilize BookManager
READ/DOS. The BookManager user may experience slow response time
when operating in a constrained memory environment or performing a
substantial amount of I/O with old I/O technology.  The more memory
the product has available the better the performance will appear.
 
If creating notes in books that reside on a floppy drive or a LAN,
make sure to include a -newnotefiledirectory statement in your
READ/DOS profile.  This statement tells READ/DOS where to create
the file containing the note instead of using the current directory.
